There is no longer a display with buttons below it so I decided to move the entire unit inside the kegerator. The Arudino and ZigBee sensors are housed in a waterproof tackle box with an Ethernet and power cable running inside via drilled holes. The housing is hanging from the inside of the door. I also added three LEDs so I could have some status showing on the board itself without having to ask the Arduino the status via the ZigBee.